IFC building model
Schema: "IFC4X3_ADD2"
Description: "ViewDefinition [CoordinationView, QuantityTakeOffAddOnView]"
Description: "RevitIdentifiers [ContentGUID: a39d7d3d-2244-4ca6-86a1-f4f79e1e0dbb, VersionGUID: cb7a33d1-5bd0-46f8-a1ec-7c482799e962, NumberOfSaves: 87]"
Description: "CoordinateReference [CoordinateBase: Survey Point, ProjectSite: Default Site]"
File name: "RK-Bridge-RVT-CIADD.ifc"
Time stamp: "2026-02-15T15:48:53+02:00"
Preprocessor: "ODA SDAI 25.12"
Originating system: "Autodesk - Revit 26.4.0.32 (ENU) - 26.4.10.8"
Application: "Autodesk Revit 2026 (ENU)" version "2026" identifier "Revit" by Organization "Autodesk Revit 2026 (ENU)"

People and organizations
  Person "Raido" "Puust" of Organization (no name given)
  Owner history of Person "Raido" "Puust" of Organization (no name given) | application "Autodesk Revit 2026 (ENU)" version "2026" identifier "Revit" by Organization "Autodesk Revit 2026 (ENU)" | change NOCHANGE | created 1771163302 (2026-02-15T13:48:22Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)

Spatial structure
IFCPROJECT "2026-02" | long name "RK - Bridge" | phase "Project Status"
  IFCSITE "Ehitajate road T2" | latitude 42° 21′ 31.401672″ | longitude -71° 3′ 24.318237″ | elevation above sea level 0.
    IFCBRIDGE "Bridge 01" | long name "Bridge 01"
      IFCBRIDGEPART "Level 1" | long name "Level 1"
        contains 4 elements
          1 x IFCWALL | type IFCWALLTYPE "Direct Shape:Abutment 2" | RETAININGWALL | names: "Direct Shape:Abutment 2:423047" | material: "Material __RGBA_0.682_0.671_0.651_1.000" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, CIADD_Admin, Qto_BodyGeometryValidation, Qto_WallBaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "Direct Shape:Abutment 1" | RETAININGWALL | names: "Direct Shape:Abutment 1:423061" | material: "Material __RGBA_0.682_0.671_0.651_1.000" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, CIADD_Admin, Qto_BodyGeometryValidation, Qto_WallBaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Direct Shape:Pier 1" | PIERSTEM | names: "Direct Shape:Pier 1:423083" | material: "Material __RGBA_0.682_0.671_0.651_1.000" | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn, CIADD_Admin, Qto_BodyGeometryValidation, Qto_ColumnBaseQuantities
          1 x IFCDEEPFOUNDATION | type IFCDEEPFOUNDATIONTYPE "Direct Shape:Foundation 1" | names: "Direct Shape:Foundation 1:423095" | material: "Material __RGBA_0.682_0.671_0.651_1.000" | property sets: Pset_EnvironmentalImpactIndicators, Qto_BodyGeometryValidation
      IFCBRIDGEPART "Level 2" | long name "Level 2"
        contains 26 elements
          1 x IFCSLAB | type IFCSLABTYPE "423043" | FLOOR | names: "423043" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, CIADD_Admin, Qto_BodyGeometryValidation, Qto_SlabBaseQuantities
          1 x IFCBEARING | type IFCBEARINGTYPE "Direct Shape:Bearing 1 (1)" | ELASTOMERIC | names: "Direct Shape:Bearing 1 (1):423051" | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000") | property sets: Pset_EnvironmentalImpactIndicators, Qto_BodyGeometryValidation
          1 x IFCBEARING | type IFCBEARINGTYPE "Direct Shape:Bearing 1 (2)" | ELASTOMERIC | names: "Direct Shape:Bearing 1 (2):423053" | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000") | property sets: Pset_EnvironmentalImpactIndicators, Qto_BodyGeometryValidation
          1 x IFCBEARING | type IFCBEARINGTYPE "Direct Shape:Bearing 1 (3)" | ELASTOMERIC | names: "Direct Shape:Bearing 1 (3):423055" | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000") | property sets: Pset_EnvironmentalImpactIndicators, Qto_BodyGeometryValidation
          1 x IFCBEARING | type IFCBEARINGTYPE "Direct Shape:Bearing 1 (4)" | ELASTOMERIC | names: "Direct Shape:Bearing 1 (4):423057" | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000") | property sets: Pset_EnvironmentalImpactIndicators, Qto_BodyGeometryValidation
          1 x IFCBEARING | type IFCBEARINGTYPE "Direct Shape:Bearing 1 (5)" | ELASTOMERIC | names: "Direct Shape:Bearing 1 (5):423059" | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000") | property sets: Pset_EnvironmentalImpactIndicators, Qto_BodyGeometryValidation
          1 x IFCBEARING | type IFCBEARINGTYPE "Direct Shape:Bearing 1 (6)" | ELASTOMERIC | names: "Direct Shape:Bearing 1 (6):423063" | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000") | property sets: Pset_EnvironmentalImpactIndicators, Qto_BodyGeometryValidation
          1 x IFCBEARING | type IFCBEARINGTYPE "Direct Shape:Bearing 1 (7)" | ELASTOMERIC | names: "Direct Shape:Bearing 1 (7):423065" | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000") | property sets: Pset_EnvironmentalImpactIndicators, Qto_BodyGeometryValidation
          1 x IFCBEARING | type IFCBEARINGTYPE "Direct Shape:Bearing 1 (8)" | ELASTOMERIC | names: "Direct Shape:Bearing 1 (8):423067" | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000") | property sets: Pset_EnvironmentalImpactIndicators, Qto_BodyGeometryValidation
          1 x IFCBEARING | type IFCBEARINGTYPE "Direct Shape:Bearing 1 (9)" | ELASTOMERIC | names: "Direct Shape:Bearing 1 (9):423069" | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000") | property sets: Pset_EnvironmentalImpactIndicators, Qto_BodyGeometryValidation
          1 x IFCBEARING | type IFCBEARINGTYPE "Direct Shape:Bearing 1 (10)" | ELASTOMERIC | names: "Direct Shape:Bearing 1 (10):423071" | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000") | property sets: Pset_EnvironmentalImpactIndicators, Qto_BodyGeometryValidation
          10 x IFCBEAM | GIRDER_SEGMENT | names: "423072", "423073", "423074" (+7 more) | material: "Bridge Concrete" | property sets: Qto_BeamBaseQuantities, Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BodyGeometryValidation
          1 x IFCBEARING | type IFCBEARINGTYPE "Direct Shape:Bearing 1 (11)" | ELASTOMERIC | names: "Direct Shape:Bearing 1 (11):423085" | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000") | property sets: Pset_EnvironmentalImpactIndicators, Qto_BodyGeometryValidation
          1 x IFCBEARING | type IFCBEARINGTYPE "Direct Shape:Bearing 1 (12)" | ELASTOMERIC | names: "Direct Shape:Bearing 1 (12):423087" | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000") | property sets: Pset_EnvironmentalImpactIndicators, Qto_BodyGeometryValidation
          1 x IFCBEARING | type IFCBEARINGTYPE "Direct Shape:Bearing 1 (13)" | ELASTOMERIC | names: "Direct Shape:Bearing 1 (13):423089" | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000") | property sets: Pset_EnvironmentalImpactIndicators, Qto_BodyGeometryValidation
          1 x IFCBEARING | type IFCBEARINGTYPE "Direct Shape:Bearing 1 (14)" | ELASTOMERIC | names: "Direct Shape:Bearing 1 (14):423091" | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000") | property sets: Pset_EnvironmentalImpactIndicators, Qto_BodyGeometryValidation
          1 x IFCBEARING | type IFCBEARINGTYPE "Direct Shape:Bearing 1" | ELASTOMERIC | names: "Direct Shape:Bearing 1:423093" | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000") | property sets: Pset_EnvironmentalImpactIndicators, Qto_BodyGeometryValidation

Types
  IFCWALLTYPE "Direct Shape:Abutment 2" | RETAININGWALL | 1 occurrence | material: "Material __RGBA_0.682_0.671_0.651_1.000"
  IFCWALLTYPE "Direct Shape:Abutment 1" | RETAININGWALL | 1 occurrence | material: "Material __RGBA_0.682_0.671_0.651_1.000"
  IFCCOLUMNTYPE "Direct Shape:Pier 1" | PIERSTEM | 1 occurrence | material: "Material __RGBA_0.682_0.671_0.651_1.000"
  IFCDEEPFOUNDATIONTYPE "Direct Shape:Foundation 1" | 1 occurrence | material: "Material __RGBA_0.682_0.671_0.651_1.000"
  IFCSLABTYPE "423043" | FLOOR | 1 occurrence
  IFCBEARINGTYPE "Direct Shape:Bearing 1 (1)" | ELASTOMERIC | 1 occurrence | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000")
  IFCBEARINGTYPE "Direct Shape:Bearing 1 (2)" | ELASTOMERIC | 1 occurrence | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000")
  IFCBEARINGTYPE "Direct Shape:Bearing 1 (3)" | ELASTOMERIC | 1 occurrence | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000")
  IFCBEARINGTYPE "Direct Shape:Bearing 1 (4)" | ELASTOMERIC | 1 occurrence | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000")
  IFCBEARINGTYPE "Direct Shape:Bearing 1 (5)" | ELASTOMERIC | 1 occurrence | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000")
  IFCBEARINGTYPE "Direct Shape:Bearing 1 (6)" | ELASTOMERIC | 1 occurrence | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000")
  IFCBEARINGTYPE "Direct Shape:Bearing 1 (7)" | ELASTOMERIC | 1 occurrence | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000")
  IFCBEARINGTYPE "Direct Shape:Bearing 1 (8)" | ELASTOMERIC | 1 occurrence | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000")
  IFCBEARINGTYPE "Direct Shape:Bearing 1 (9)" | ELASTOMERIC | 1 occurrence | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000")
  IFCBEARINGTYPE "Direct Shape:Bearing 1 (10)" | ELASTOMERIC | 1 occurrence | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000")
  IFCBEARINGTYPE "Direct Shape:Bearing 1 (11)" | ELASTOMERIC | 1 occurrence | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000")
  IFCBEARINGTYPE "Direct Shape:Bearing 1 (12)" | ELASTOMERIC | 1 occurrence | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000")
  IFCBEARINGTYPE "Direct Shape:Bearing 1 (13)" | ELASTOMERIC | 1 occurrence | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000")
  IFCBEARINGTYPE "Direct Shape:Bearing 1 (14)" | ELASTOMERIC | 1 occurrence | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000")
  IFCBEARINGTYPE "Direct Shape:Bearing 1" | ELASTOMERIC | 1 occurrence | material: constituents ("Material __RGBA_0.682_0.671_0.651_1.000": "Material __RGBA_0.682_0.671_0.651_1.000", "Material __RGBA_0.263_0.263_0.251_1.000": "Material __RGBA_0.263_0.263_0.251_1.000")

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 2 objects (1 IFCBRIDGE, 1 IFCSITE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 2 objects (2 IFCBRIDGEPART)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "8mm Head" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 11 objects (10 IFCBEAM, 1 IFCSLAB)
    Reference = "" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCWALL)
    Reference = "Abutment 2" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBEARING)
    Reference = "Bearing 1 (1)" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBEARING)
    Reference = "Bearing 1 (2)" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBEARING)
    Reference = "Bearing 1 (3)" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBEARING)
    Reference = "Bearing 1 (4)" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBEARING)
    Reference = "Bearing 1 (5)" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCWALL)
    Reference = "Abutment 1" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators: 12 more contents on 12 objects not shown
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    PitchAngle = 0.90595119311016636 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "" (IFCIDENTIFIER)
  CIADD_Admin | properties | on 1 object (1 IFCSLAB)
    AN010_Name = "Cast-in-place concrete plate" (IFCTEXT)
    AN112_Type = "ULK10" (IFCTEXT)
    AN114_ID = "ULK10_01" (IFCTEXT)
    AN130_System = "Superstructure of ceiling system" (IFCTEXT)
    AN132_SystemType = "C13" (IFCTEXT)
    AN134_SystemID = "C1301" (IFCTEXT)
    AN160_Subsystem = "General beam structure" (IFCTEXT)
    AN162_SubsystemType = "BC01" (IFCTEXT)
    AN164_SubsystemID = "BC0101" (IFCTEXT)
    AR360_UniqueID = "C1301.BC0101.ULK10_01" (IFCTEXT)
    PU280_MaterialType = "Concrete" (IFCTEXT)
    VP198_QuantityUnit = "m3" (IFCTEXT)
    VP199_QuantityValue = "180.6" (IFCTEXT)
  CIADD_Admin | properties | on 1 object (1 IFCWALL)
    AN130_System = "Above ground wall system" (IFCTEXT)
    AN132_SystemType = "B12" (IFCTEXT)
    AN134_SystemID = "B1201" (IFCTEXT)
    AN160_Subsystem = "General foundation and base construction" (IFCTEXT)
    AN162_SubsystemType = "CJ01" (IFCTEXT)
    AN164_SubsystemID = "CJ0101" (IFCTEXT)
    AR360_UniqueID = "B1201.CJ0101.ULJ10_01" (IFCTEXT)
    VP198_QuantityUnit = "m3" (IFCTEXT)
  CIADD_Admin | properties | on 1 object (1 IFCWALL)
    AN130_System = "Above ground wall system" (IFCTEXT)
    AN132_SystemType = "B12" (IFCTEXT)
    AN134_SystemID = "B1201" (IFCTEXT)
    AN160_Subsystem = "General foundation and base construction" (IFCTEXT)
    AN162_SubsystemType = "CJ01" (IFCTEXT)
    AN164_SubsystemID = "CJ0101" (IFCTEXT)
    AR360_UniqueID = "B1201.CJ0101.ULJ10_02" (IFCTEXT)
    VP198_QuantityUnit = "m3" (IFCTEXT)
  CIADD_Admin | properties | on 1 object (1 IFCCOLUMN)
    AN010_Name = "Cast-in-place concrete column" (IFCTEXT)
    AN112_Type = "ULD10" (IFCTEXT)
    AN114_ID = "ULD10_01" (IFCTEXT)
    AN130_System = "Above ground wall system" (IFCTEXT)
    AN132_SystemType = "B12" (IFCTEXT)
    AN134_SystemID = "B1201" (IFCTEXT)
    AN160_Subsystem = "General wall construction" (IFCTEXT)
    AN162_SubsystemType = "BD01" (IFCTEXT)
    AN164_SubsystemID = "BD0101" (IFCTEXT)
    AR360_UniqueID = "B1201.BD0101.ULD10_01" (IFCTEXT)
    PU280_MaterialType = "Concrete" (IFCTEXT)
    VP198_QuantityUnit = "m3" (IFCTEXT)
    VP199_QuantityValue = "173.9" (IFCTEXT)
  Qto_BodyGeometryValidation | quantities | on 3 objects (3 IFCBEARING)
    NetSurfaceArea = 1.6541704977742417 [SQUARE_METRE]
    NetVolume = 0.037765081506902741 [CUBIC_METRE]
  Qto_BodyGeometryValidation | quantities | on 2 objects (2 IFCBEARING)
    NetSurfaceArea = 1.6541704977742417 [SQUARE_METRE]
    NetVolume = 0.037765081506902783 [CUBIC_METRE]
  Qto_BodyGeometryValidation | quantities | on 2 objects (2 IFCBEARING)
    NetSurfaceArea = 1.6542408191054749 [SQUARE_METRE]
    NetVolume = 0.037773809901811915 [CUBIC_METRE]
  Qto_BodyGeometryValidation | quantities | on 1 object (1 IFCSLAB)
    NetSurfaceArea = 1235.7002708474881 [SQUARE_METRE]
    NetVolume = 180.62834933579975 [CUBIC_METRE]
  Qto_BodyGeometryValidation | quantities | on 1 object (1 IFCWALL)
    NetSurfaceArea = 696.66832935295758 [SQUARE_METRE]
    NetVolume = 313.12173499148031 [CUBIC_METRE]
  Qto_BodyGeometryValidation | quantities | on 1 object (1 IFCBEARING)
    NetSurfaceArea = 1.6542408191054749 [SQUARE_METRE]
    NetVolume = 0.037773809901811964 [CUBIC_METRE]
  Qto_BodyGeometryValidation | quantities | on 1 object (1 IFCBEARING)
    NetSurfaceArea = 1.6542408191054749 [SQUARE_METRE]
    NetVolume = 0.037773809901811957 [CUBIC_METRE]
  Qto_BodyGeometryValidation | quantities | on 1 object (1 IFCWALL)
    NetSurfaceArea = 699.0417288538813 [SQUARE_METRE]
    NetVolume = 313.32096242712043 [CUBIC_METRE]
  Qto_BodyGeometryValidation: 18 more contents on 18 objects not shown
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Length = 35729.289174488869 [MILLI METRE]
    NetVolume = 180.62834933579975 [CUBIC_METRE]
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALL)
    Reference = "Abutment 2" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALL)
    Reference = "Abutment 1" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Abutment 2" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Abutment 1" (IFCIDENTIFIER)
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    NetVolume = 313.12173499148031 [CUBIC_METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    NetVolume = 313.32096242712043 [CUBIC_METRE]
  Qto_BeamBaseQuantities | quantities | on 10 objects (10 IFCBEAM)
    GrossSurfaceArea = 0. [SQUARE_METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Slope = 89.191625210386036 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Slope = 89.191601571321968 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Slope = 89.191577971708199 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Slope = 89.186848973302887 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Slope = 89.186872624074965 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Slope = 89.191617976654996 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Slope = 89.191594342029688 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Slope = 89.191570753228575 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon: 2 more contents on 2 objects not shown
  Pset_ReinforcementBarPitchOfBeam | properties | on 10 objects (10 IFCBEAM)
    Reference = "" (IFCLABEL)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Pier 1" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfColumn | properties | on 1 object (1 IFCCOLUMN)
    Reference = "Pier 1" (IFCLABEL)
  Qto_ColumnBaseQuantities | quantities | on 1 object (1 IFCCOLUMN)
    NetSurfaceArea = 286.32594433547456 [SQUARE_METRE]
    NetVolume = 173.89071604198745 [CUBIC_METRE]
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBRIDGEPART)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "8mm Head" (IFCIDENTIFIER)