IFC building model
Schema: "IFC4X3"
Description: "ViewDefinition [CoordinationView]"
Description: "RevitIdentifiers [VersionGUID: bf8fc2c9-0ae9-44e4-9809-1235c9803230, NumberOfSaves: 49]"
Description: "CoordinateReference [CoordinateBase: Shared Coordinates, ProjectSite: Default Site]"
File name: "Project Number"
Time stamp: "2024-04-19T12:30:52+02:00"
Preprocessor: "ODA SDAI 24.6"
Originating system: "Autodesk Revit 24.2.0.63 (ENU) - IFC 24.2.0.63"
Application: "Autodesk Revit 2024 (ENU)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENU)"

People and organizations
  Person "Raido" "Puust" of Organization (no name given)
  Owner history of Person "Raido" "Puust" of Organization (no name given) | application "Autodesk Revit 2024 (ENU)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENU)" | change NOCHANGE | created 1713444474 (2024-04-18T12:47:54Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  AREADENSITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 59° 23′ 50.806648″ | longitude 24° 40′ 20.882507″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "59.3974462911838", "24.6724673632588"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 0.
        contains 4 elements
          1 x IFCSLAB | type IFCSLABTYPE "Direct Shape:Abutment 2" | object type "Direct Shape:Abutment 2" | names: "Direct Shape:Abutment 2:423047" | material: "Material __RGBA_0.682_0.671_0.651_1.000" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, A010_AdminElement, Other, Dimensions
          1 x IFCSLAB | type IFCSLABTYPE "Direct Shape:Abutment 1" | object type "Direct Shape:Abutment 1" | names: "Direct Shape:Abutment 1:423061" | material: "Material __RGBA_0.682_0.671_0.651_1.000" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, A010_AdminElement, Other, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Direct Shape:Pier 1" | object type "Direct Shape:Pier 1" | names: "Direct Shape:Pier 1:423083" | material: "Material __RGBA_0.682_0.671_0.651_1.000" | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn, A010_AdminElement, Other, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Direct Shape:Foundation 1" | object type "Direct Shape:Foundation 1" | names: "Direct Shape:Foundation 1:423095" | material: "Material __RGBA_0.682_0.671_0.651_1.000" | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn, A010_AdminElement, Other, Dimensions
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | object type "Level:8mm Head" | elevation 3000.
        contains 26 elements
          1 x IFCSLAB | type IFCSLABTYPE "423043" | FLOOR | names: "423043" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, A010_AdminElement, Other, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (1)" | object type "Direct Shape:Bearing 1 (1)" | names: "Direct Shape:Bearing 1 (1):423051" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (2)" | object type "Direct Shape:Bearing 1 (2)" | names: "Direct Shape:Bearing 1 (2):423053" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (3)" | object type "Direct Shape:Bearing 1 (3)" | names: "Direct Shape:Bearing 1 (3):423055" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (4)" | object type "Direct Shape:Bearing 1 (4)" | names: "Direct Shape:Bearing 1 (4):423057" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (5)" | object type "Direct Shape:Bearing 1 (5)" | names: "Direct Shape:Bearing 1 (5):423059" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (6)" | object type "Direct Shape:Bearing 1 (6)" | names: "Direct Shape:Bearing 1 (6):423063" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (7)" | object type "Direct Shape:Bearing 1 (7)" | names: "Direct Shape:Bearing 1 (7):423065" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (8)" | object type "Direct Shape:Bearing 1 (8)" | names: "Direct Shape:Bearing 1 (8):423067" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (9)" | object type "Direct Shape:Bearing 1 (9)" | names: "Direct Shape:Bearing 1 (9):423069" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (10)" | object type "Direct Shape:Bearing 1 (10)" | names: "Direct Shape:Bearing 1 (10):423071" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "423072" | names: "423072" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "423073" | names: "423073" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "423074" | names: "423074" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "423075" | names: "423075" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "423076" | names: "423076" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "423077" | names: "423077" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "423078" | names: "423078" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "423079" | names: "423079" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "423080" | names: "423080" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "423081" | names: "423081" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (11)" | object type "Direct Shape:Bearing 1 (11)" | names: "Direct Shape:Bearing 1 (11):423085" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (12)" | object type "Direct Shape:Bearing 1 (12)" | names: "Direct Shape:Bearing 1 (12):423087" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (13)" | object type "Direct Shape:Bearing 1 (13)" | names: "Direct Shape:Bearing 1 (13):423089" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (14)" | object type "Direct Shape:Bearing 1 (14)" | names: "Direct Shape:Bearing 1 (14):423091" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1" | object type "Direct Shape:Bearing 1" | names: "Direct Shape:Bearing 1:423093" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, A010_AdminElement, Other, Dimensions, General

Types
  IFCSLABTYPE "Direct Shape:Abutment 2" | 1 occurrence | material: "Material __RGBA_0.682_0.671_0.651_1.000" | property sets: Other, Identity Data, Pset_SlabCommon
  IFCSLABTYPE "Direct Shape:Abutment 1" | 1 occurrence | material: "Material __RGBA_0.682_0.671_0.651_1.000" | property sets: Other, Identity Data, Pset_SlabCommon
  IFCCOLUMNTYPE "Direct Shape:Pier 1" | COLUMN | 1 occurrence | material: "Material __RGBA_0.682_0.671_0.651_1.000" | property sets: Other, Identity Data, Pset_ColumnCommon
  IFCCOLUMNTYPE "Direct Shape:Foundation 1" | COLUMN | 1 occurrence | material: "Material __RGBA_0.682_0.671_0.651_1.000" | property sets: Other, Identity Data, Pset_ColumnCommon
  IFCSLABTYPE "423043" | FLOOR | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (1)" | 1 occurrence | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (2)" | 1 occurrence | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (3)" | 1 occurrence | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (4)" | 1 occurrence | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (5)" | 1 occurrence | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (6)" | 1 occurrence | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (7)" | 1 occurrence | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (8)" | 1 occurrence | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (9)" | 1 occurrence | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (10)" | 1 occurrence | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "423072" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "423073" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "423074" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "423075" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "423076" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "423077" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "423078" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "423079" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "423080" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "423081" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (11)" | 1 occurrence | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (12)" | 1 occurrence | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (13)" | 1 occurrence | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1 (14)" | 1 occurrence | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Direct Shape:Bearing 1" | 1 occurrence | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "8mm Head" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 11 objects (10 IFCBUILDINGELEMENTPROXY, 1 IFCSLAB)
    Reference = "" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCSLAB)
    Reference = "Abutment 2" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Bearing 1 (1)" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Bearing 1 (2)" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Bearing 1 (3)" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Bearing 1 (4)" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Bearing 1 (5)" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCSLAB)
    Reference = "Abutment 1" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators: 12 more contents on 12 objects not shown
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Abutment 2" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Abutment 1" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    PitchAngle = 0.90595119311016636 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Abutment 2" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Abutment 1" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
  A010_AdminElement | properties | on 1 object (1 IFCSLAB)
    AC155_SysteemKlassKood = "C" (IFCTEXT)
    AC156_SysteemTyypKood = "C50" (IFCTEXT)
    AC157_SysteemID = "C5001" (IFCTEXT)
    AC160_SysteemKlassNimi = "Vahelaesüsteem" (IFCTEXT)
    AC161_SysteemTyypNimi = "Silla pealisehituse süsteem" (IFCTEXT)
    AC165_OsasysteemKlassKood = "BC" (IFCTEXT)
    AC166_OsasysteemTyypKood = "BC10" (IFCTEXT)
    AC167_OsasysteemID = "BC1001" (IFCTEXT)
    AC170_OsasysteemKlassNimi = "Talakonstruktsioon" (IFCTEXT)
    AC171_OsaSysteemTyypNimi = "Massiivplaadi konstruktsioon" (IFCTEXT)
    AC175_KomponentKlassKood = "ULK" (IFCTEXT)
    AC176_KomponentTyypKood = "ULK21" (IFCTEXT)
    AC177_KomponentID = "ULK01" (IFCTEXT)
    AC180_KomponentKlassNimi = "Plaat" (IFCTEXT)
    AC181_KomponentTyypNimi = "Betoonvalust plaat" (IFCTEXT)
    AR340_Viitetunnus = "ULK01%ULK21" (IFCTEXT)
    AR360_UnikaalneID = "C5001.BC1001.ULK01%ULK21" (IFCTEXT)
  A010_AdminElement | properties | on 1 object (1 IFCSLAB)
    AC155_SysteemKlassKood = "B" (IFCTEXT)
    AC156_SysteemTyypKood = "B32" (IFCTEXT)
    AC157_SysteemID = "B3201" (IFCTEXT)
    AC160_SysteemKlassNimi = "Seinasüsteem" (IFCTEXT)
    AC161_SysteemTyypNimi = "Toeseina süsteem" (IFCTEXT)
    AC165_OsasysteemKlassKood = "CJ" (IFCTEXT)
    AC166_OsasysteemTyypKood = "CJ10" (IFCTEXT)
    AC167_OsasysteemID = "CJ1001" (IFCTEXT)
    AC170_OsasysteemKlassNimi = "Vundamendi ja aluse konstruktsioon" (IFCTEXT)
    AC171_OsaSysteemTyypNimi = "Tugiseina ehitus" (IFCTEXT)
    AC175_KomponentKlassKood = "ULJ" (IFCTEXT)
    AC176_KomponentTyypKood = "ULJ10" (IFCTEXT)
    AC177_KomponentID = "ULJ01" (IFCTEXT)
    AC180_KomponentKlassNimi = "Kaldtugi" (IFCTEXT)
    AC181_KomponentTyypNimi = "Kaldasammas" (IFCTEXT)
    AR340_Viitetunnus = "ULJ01%ULJ10" (IFCTEXT)
    AR360_UnikaalneID = "B3201.CJ1001.ULJ01%ULJ10" (IFCTEXT)
  A010_AdminElement | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AC155_SysteemKlassKood = "C" (IFCTEXT)
    AC156_SysteemTyypKood = "C50" (IFCTEXT)
    AC157_SysteemID = "C5001" (IFCTEXT)
    AC160_SysteemKlassNimi = "Vahelaesüsteem" (IFCTEXT)
    AC161_SysteemTyypNimi = "Silla pealisehituse süsteem" (IFCTEXT)
    AC165_OsasysteemKlassKood = "BC" (IFCTEXT)
    AC166_OsasysteemTyypKood = "BC20" (IFCTEXT)
    AC167_OsasysteemID = "BC2001" (IFCTEXT)
    AC170_OsasysteemKlassNimi = "Talakonstruktsioon" (IFCTEXT)
    AC171_OsaSysteemTyypNimi = "Tala konstruktsioon" (IFCTEXT)
    AC175_KomponentKlassKood = "UPA" (IFCTEXT)
    AC176_KomponentTyypKood = "UPA70" (IFCTEXT)
    AC177_KomponentID = "UPA12" (IFCTEXT)
    AC180_KomponentKlassNimi = "Laagerdus" (IFCTEXT)
    AC181_KomponentTyypNimi = "Elastomeerne laager" (IFCTEXT)
    AR340_Viitetunnus = "UPA12%UPA70" (IFCTEXT)
    AR360_UnikaalneID = "C5001.BC2001.UPA12%UPA70" (IFCTEXT)
  A010_AdminElement | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AC155_SysteemKlassKood = "C" (IFCTEXT)
    AC156_SysteemTyypKood = "C50" (IFCTEXT)
    AC157_SysteemID = "C5001" (IFCTEXT)
    AC160_SysteemKlassNimi = "Vahelaesüsteem" (IFCTEXT)
    AC161_SysteemTyypNimi = "Silla pealisehituse süsteem" (IFCTEXT)
    AC165_OsasysteemKlassKood = "BC" (IFCTEXT)
    AC166_OsasysteemTyypKood = "BC20" (IFCTEXT)
    AC167_OsasysteemID = "BC2001" (IFCTEXT)
    AC170_OsasysteemKlassNimi = "Talakonstruktsioon" (IFCTEXT)
    AC171_OsaSysteemTyypNimi = "Tala konstruktsioon" (IFCTEXT)
    AC175_KomponentKlassKood = "UPA" (IFCTEXT)
    AC176_KomponentTyypKood = "UPA70" (IFCTEXT)
    AC177_KomponentID = "UPA11" (IFCTEXT)
    AC180_KomponentKlassNimi = "Laagerdus" (IFCTEXT)
    AC181_KomponentTyypNimi = "Elastomeerne laager" (IFCTEXT)
    AR340_Viitetunnus = "UPA11%UPA70" (IFCTEXT)
    AR360_UnikaalneID = "C5001.BC2001.UPA11%UPA70" (IFCTEXT)
  A010_AdminElement | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AC155_SysteemKlassKood = "C" (IFCTEXT)
    AC156_SysteemTyypKood = "C50" (IFCTEXT)
    AC157_SysteemID = "C5001" (IFCTEXT)
    AC160_SysteemKlassNimi = "Vahelaesüsteem" (IFCTEXT)
    AC161_SysteemTyypNimi = "Silla pealisehituse süsteem" (IFCTEXT)
    AC165_OsasysteemKlassKood = "BC" (IFCTEXT)
    AC166_OsasysteemTyypKood = "BC20" (IFCTEXT)
    AC167_OsasysteemID = "BC2001" (IFCTEXT)
    AC170_OsasysteemKlassNimi = "Talakonstruktsioon" (IFCTEXT)
    AC171_OsaSysteemTyypNimi = "Tala konstruktsioon" (IFCTEXT)
    AC175_KomponentKlassKood = "UPA" (IFCTEXT)
    AC176_KomponentTyypKood = "UPA70" (IFCTEXT)
    AC177_KomponentID = "UPA13" (IFCTEXT)
    AC180_KomponentKlassNimi = "Laagerdus" (IFCTEXT)
    AC181_KomponentTyypNimi = "Elastomeerne laager" (IFCTEXT)
    AR340_Viitetunnus = "UPA13%UPA70" (IFCTEXT)
    AR360_UnikaalneID = "C5001.BC2001.UPA13%UPA70" (IFCTEXT)
  A010_AdminElement | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AC155_SysteemKlassKood = "C" (IFCTEXT)
    AC156_SysteemTyypKood = "C50" (IFCTEXT)
    AC157_SysteemID = "C5001" (IFCTEXT)
    AC160_SysteemKlassNimi = "Vahelaesüsteem" (IFCTEXT)
    AC161_SysteemTyypNimi = "Silla pealisehituse süsteem" (IFCTEXT)
    AC165_OsasysteemKlassKood = "BC" (IFCTEXT)
    AC166_OsasysteemTyypKood = "BC20" (IFCTEXT)
    AC167_OsasysteemID = "BC2001" (IFCTEXT)
    AC170_OsasysteemKlassNimi = "Talakonstruktsioon" (IFCTEXT)
    AC171_OsaSysteemTyypNimi = "Tala konstruktsioon" (IFCTEXT)
    AC175_KomponentKlassKood = "UPA" (IFCTEXT)
    AC176_KomponentTyypKood = "UPA70" (IFCTEXT)
    AC177_KomponentID = "UPA14" (IFCTEXT)
    AC180_KomponentKlassNimi = "Laagerdus" (IFCTEXT)
    AC181_KomponentTyypNimi = "Elastomeerne laager" (IFCTEXT)
    AR340_Viitetunnus = "UPA14%UPA70" (IFCTEXT)
    AR360_UnikaalneID = "C5001.BC2001.UPA14%UPA70" (IFCTEXT)
  A010_AdminElement | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AC155_SysteemKlassKood = "C" (IFCTEXT)
    AC156_SysteemTyypKood = "C50" (IFCTEXT)
    AC157_SysteemID = "C5001" (IFCTEXT)
    AC160_SysteemKlassNimi = "Vahelaesüsteem" (IFCTEXT)
    AC161_SysteemTyypNimi = "Silla pealisehituse süsteem" (IFCTEXT)
    AC165_OsasysteemKlassKood = "BC" (IFCTEXT)
    AC166_OsasysteemTyypKood = "BC20" (IFCTEXT)
    AC167_OsasysteemID = "BC2001" (IFCTEXT)
    AC170_OsasysteemKlassNimi = "Talakonstruktsioon" (IFCTEXT)
    AC171_OsaSysteemTyypNimi = "Tala konstruktsioon" (IFCTEXT)
    AC175_KomponentKlassKood = "UPA" (IFCTEXT)
    AC176_KomponentTyypKood = "UPA70" (IFCTEXT)
    AC177_KomponentID = "UPA15" (IFCTEXT)
    AC180_KomponentKlassNimi = "Laagerdus" (IFCTEXT)
    AC181_KomponentTyypNimi = "Elastomeerne laager" (IFCTEXT)
    AR340_Viitetunnus = "UPA15%UPA70" (IFCTEXT)
    AR360_UnikaalneID = "C5001.BC2001.UPA15%UPA70" (IFCTEXT)
  A010_AdminElement | properties | on 1 object (1 IFCSLAB)
    AC155_SysteemKlassKood = "B" (IFCTEXT)
    AC156_SysteemTyypKood = "B32" (IFCTEXT)
    AC157_SysteemID = "B3201" (IFCTEXT)
    AC160_SysteemKlassNimi = "Seinasüsteem" (IFCTEXT)
    AC161_SysteemTyypNimi = "Toeseina süsteem" (IFCTEXT)
    AC165_OsasysteemKlassKood = "CJ" (IFCTEXT)
    AC166_OsasysteemTyypKood = "CJ10" (IFCTEXT)
    AC167_OsasysteemID = "CJ1001" (IFCTEXT)
    AC170_OsasysteemKlassNimi = "Vundamendi ja aluse konstruktsioon" (IFCTEXT)
    AC171_OsaSysteemTyypNimi = "Tugiseina ehitus" (IFCTEXT)
    AC175_KomponentKlassKood = "ULJ" (IFCTEXT)
    AC176_KomponentTyypKood = "ULJ10" (IFCTEXT)
    AC177_KomponentID = "ULJ02" (IFCTEXT)
    AC180_KomponentKlassNimi = "Kaldtugi" (IFCTEXT)
    AC181_KomponentTyypNimi = "Kaldasammas" (IFCTEXT)
    AR340_Viitetunnus = "ULJ02%ULJ10" (IFCTEXT)
    AR360_UnikaalneID = "B3201.CJ1001.ULJ02%ULJ10" (IFCTEXT)
  A010_AdminElement: 22 more contents on 22 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Bearing 1 (1)" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Bearing 1 (2)" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Bearing 1 (3)" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Bearing 1 (4)" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Bearing 1 (5)" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Bearing 1 (6)" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Bearing 1 (7)" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 10 more contents on 9 objects not shown
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Pier 1" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Foundation 1" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_ReinforcementBarPitchOfColumn | properties | on 1 object (1 IFCCOLUMN)
    Reference = "Pier 1" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 1 object (1 IFCCOLUMN)
    Reference = "Foundation 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "8mm Head" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 2 (IFCCOUNTMEASURE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Project Information" (IFCIDENTIFIER)
  A001_AdminEhitis | properties | on 1 object (1 IFCBUILDING)
    AC135_EhKompleksKlassKood = "R" (IFCTEXT)
    AC140_EhKompleksKlassNimi = "Liikluskompleks" (IFCTEXT)
    AC145_EhitisKlassKood = "RK" (IFCTEXT)
    AC150_EhitisKlassNimi = "Sild" (IFCTEXT)
  Other | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY)
    Category = "Bridge Framing: Girders" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "8mm Head" (IFCLABEL)
    Type Id = "333" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCSLAB)
    Category = "Bridge Decks" (IFCLABEL)
  Other | properties | on 1 object (1 IFCSLAB)
    Category = "Abutments" (IFCLABEL)
    Family = "Direct Shape" (IFCLABEL)
    Family and Type = "Direct Shape: Abutment 2" (IFCLABEL)
    Type = "Abutment 2" (IFCLABEL)
    Type Id = "423046" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Bearings" (IFCLABEL)
    Family = "Direct Shape" (IFCLABEL)
    Family and Type = "Direct Shape: Bearing 1 (1)" (IFCLABEL)
    Type = "Bearing 1 (1)" (IFCLABEL)
    Type Id = "423050" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Bearings" (IFCLABEL)
    Family = "Direct Shape" (IFCLABEL)
    Family and Type = "Direct Shape: Bearing 1 (2)" (IFCLABEL)
    Type = "Bearing 1 (2)" (IFCLABEL)
    Type Id = "423052" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Bearings" (IFCLABEL)
    Family = "Direct Shape" (IFCLABEL)
    Family and Type = "Direct Shape: Bearing 1 (3)" (IFCLABEL)
    Type = "Bearing 1 (3)" (IFCLABEL)
    Type Id = "423054" (IFCLABEL)
  Other: 19 more contents on 15 objects not shown
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 1648.43126529234 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 4648.43126529234 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY)
    [Section Dimensions] Bottom width = 711.20000000000005 (IFCLENGTHMEASURE) [MILLI METRE]
    [Section Dimensions] Depth = 1828.8000000000002 (IFCLENGTHMEASURE) [MILLI METRE]
    [Section Dimensions] T1 = 127. (IFCLENGTHMEASURE) [MILLI METRE]
    [Section Dimensions] T2 = 101.59999999999998 (IFCLENGTHMEASURE) [MILLI METRE]
    [Section Dimensions] T3 = 254. (IFCLENGTHMEASURE) [MILLI METRE]
    [Section Dimensions] T4 = 203.19999999999996 (IFCLENGTHMEASURE) [MILLI METRE]
    [Section Dimensions] Top width = 1066.8 (IFCLENGTHMEASURE) [MILLI METRE]
    [Section Dimensions] Web thickness = 203.19999999999996 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    [General] Bearing assembly height = 187.06032602761101 (IFCLENGTHMEASURE) [MILLI METRE]
    [General] Depth = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    [General] Extra height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    [General] Height = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    [General] Round bearings = FALSE (IFCBOOLEAN)
    [General] Slope at girder soffit: Longitudinal = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    [General] Slope at girder soffit: Transverse = 0.80900000000000005 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    [General] Slope at piercap: Longitudinal = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    [General] Slope at piercap: Transverse = 0.80900000000000005 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    [General] Width = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    [Masonry Plate] Masonry plate: Depth1 = 249.99999999999997 (IFCLENGTHMEASURE) [MILLI METRE]
    [Masonry Plate] Masonry plate: Depth2 = 249.99999999999997 (IFCLENGTHMEASURE) [MILLI METRE]
    [Masonry Plate] Masonry plate: Height = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    [Masonry Plate] Masonry plate: Width = 499.99999999999994 (IFCLENGTHMEASURE) [MILLI METRE]
    [Sole Plate] Sole plate: Depth1 = 249.99999999999997 (IFCLENGTHMEASURE) [MILLI METRE]
    [Sole Plate] Sole plate: Depth2 = 249.99999999999997 (IFCLENGTHMEASURE) [MILLI METRE]
    [Sole Plate] Sole plate: Height = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    [Sole Plate] Sole plate: Width = 499.99999999999994 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    [General] Bearing assembly height = 187.095239607248 (IFCLENGTHMEASURE) [MILLI METRE]
    [General] Depth = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    [General] Extra height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    [General] Height = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    [General] Round bearings = FALSE (IFCBOOLEAN)
    [General] Slope at girder soffit: Longitudinal = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    [General] Slope at girder soffit: Transverse = -0.81299999999999994 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    [General] Slope at piercap: Longitudinal = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    [General] Slope at piercap: Transverse = -0.81299999999999994 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    [General] Width = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    [Masonry Plate] Masonry plate: Depth1 = 249.99999999999997 (IFCLENGTHMEASURE) [MILLI METRE]
    [Masonry Plate] Masonry plate: Depth2 = 249.99999999999997 (IFCLENGTHMEASURE) [MILLI METRE]
    [Masonry Plate] Masonry plate: Height = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    [Masonry Plate] Masonry plate: Width = 499.99999999999994 (IFCLENGTHMEASURE) [MILLI METRE]
    [Sole Plate] Sole plate: Depth1 = 249.99999999999997 (IFCLENGTHMEASURE) [MILLI METRE]
    [Sole Plate] Sole plate: Depth2 = 249.99999999999997 (IFCLENGTHMEASURE) [MILLI METRE]
    [Sole Plate] Sole plate: Height = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    [Sole Plate] Sole plate: Width = 499.99999999999994 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCSLAB)
    [Section Dimensions] Edge thickness = 299.99999999999994 (IFCLENGTHMEASURE) [MILLI METRE]
    [Section Dimensions] Slope: Left = 1.4119999999999999 (IFCREAL)
    [Section Dimensions] Slope: Right = 1.401 (IFCREAL)
    [Section Dimensions] Tapered width: Left = 0.99999999999999989 (IFCLENGTHMEASURE) [MILLI METRE]
    [Section Dimensions] Tapered width: Right = 0.99999999999999989 (IFCLENGTHMEASURE) [MILLI METRE]
    [Section Dimensions] Thickness = 299.99999999999994 (IFCLENGTHMEASURE) [MILLI METRE]
    [Section Dimensions] Width: Left = 8500. (IFCLENGTHMEASURE) [MILLI METRE]
    [Section Dimensions] Width: Right = 8349.9999999999982 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCSLAB)
    [Ballast Wall] Height = 2015.9999999999998 (IFCLENGTHMEASURE) [MILLI METRE]
    [Ballast Wall] Thickness = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    [Geometry] Bearing centerline = 999.99999999999989 (IFCLENGTHMEASURE) [MILLI METRE]
    [Geometry] Width: Left = -8500. (IFCLENGTHMEASURE) [MILLI METRE]
    [Geometry] Width: Right = 8349.9999999999982 (IFCLENGTHMEASURE) [MILLI METRE]
    [Seat] Depth: Left = 9999.9999999999982 (IFCLENGTHMEASURE) [MILLI METRE]
    [Seat] Depth: Middle = 9999.9999999999982 (IFCLENGTHMEASURE) [MILLI METRE]
    [Seat] Depth: Right = 9999.9999999999982 (IFCLENGTHMEASURE) [MILLI METRE]
    [Seat] Width = 1600. (IFCLENGTHMEASURE) [MILLI METRE]
    [Wing Wall] Cut length: Left = 3999.9999999999995 (IFCLENGTHMEASURE) [MILLI METRE]
    [Wing Wall] Cut length: Right = 3999.9999999999995 (IFCLENGTHMEASURE) [MILLI METRE]
    [Wing Wall] Height: Left = 999.99999999999989 (IFCLENGTHMEASURE) [MILLI METRE]
    [Wing Wall] Height: Right = 999.99999999999989 (IFCLENGTHMEASURE) [MILLI METRE]
    [Wing Wall] Length: Left = 5999.9999999999991 (IFCLENGTHMEASURE) [MILLI METRE]
    [Wing Wall] Length: Right = 5999.9999999999991 (IFCLENGTHMEASURE) [MILLI METRE]
    [Wing Wall] Thickness = 299.99999999999994 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCSLAB)
    [Ballast Wall] Height = 2015.9999999999998 (IFCLENGTHMEASURE) [MILLI METRE]
    [Ballast Wall] Thickness = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    [Geometry] Bearing centerline = 999.99999999999989 (IFCLENGTHMEASURE) [MILLI METRE]
    [Geometry] Width: Left = -8349.9999999999982 (IFCLENGTHMEASURE) [MILLI METRE]
    [Geometry] Width: Right = 8500. (IFCLENGTHMEASURE) [MILLI METRE]
    [Seat] Depth: Left = 9999.9999999999982 (IFCLENGTHMEASURE) [MILLI METRE]
    [Seat] Depth: Middle = 9999.9999999999982 (IFCLENGTHMEASURE) [MILLI METRE]
    [Seat] Depth: Right = 9999.9999999999982 (IFCLENGTHMEASURE) [MILLI METRE]
    [Seat] Width = 1600. (IFCLENGTHMEASURE) [MILLI METRE]
    [Wing Wall] Cut length: Left = 3999.9999999999995 (IFCLENGTHMEASURE) [MILLI METRE]
    [Wing Wall] Cut length: Right = 3999.9999999999995 (IFCLENGTHMEASURE) [MILLI METRE]
    [Wing Wall] Height: Left = 999.99999999999989 (IFCLENGTHMEASURE) [MILLI METRE]
    [Wing Wall] Height: Right = 999.99999999999989 (IFCLENGTHMEASURE) [MILLI METRE]
    [Wing Wall] Length: Left = 5999.9999999999991 (IFCLENGTHMEASURE) [MILLI METRE]
    [Wing Wall] Length: Right = 5999.9999999999991 (IFCLENGTHMEASURE) [MILLI METRE]
    [Wing Wall] Thickness = 299.99999999999994 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCCOLUMN)
    [Cap] Depth = 2200. (IFCLENGTHMEASURE) [MILLI METRE]
    [Cap] Has rounded ends = TRUE (IFCBOOLEAN)
    [Cap] Pier height = 8153. (IFCLENGTHMEASURE) [MILLI METRE]
    [Cap] Slope: Left = 0. (IFCREAL)
    [Cap] Slope: Right = 0. (IFCREAL)
    [Cap] Tapered end: Depth = 1199.9999999999998 (IFCLENGTHMEASURE) [MILLI METRE]
    [Cap] Tapered end: Length = 2999.9999999999995 (IFCLENGTHMEASURE) [MILLI METRE]
    [Cap] Vertical offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    [Cap] Width: Back = 999.99999999999989 (IFCLENGTHMEASURE) [MILLI METRE]
    [Cap] Width: Front = 999.99999999999989 (IFCLENGTHMEASURE) [MILLI METRE]
    [Cap] Width: Left = 8500. (IFCLENGTHMEASURE) [MILLI METRE]
    [Cap] Width: Right = 8349.9999999999982 (IFCLENGTHMEASURE) [MILLI METRE]
    [Columns] Columns are round = FALSE (IFCBOOLEAN)
    [Columns] Corners are round = TRUE (IFCBOOLEAN)
    [Columns] Depth = 1799.9999999999998 (IFCLENGTHMEASURE) [MILLI METRE]
    [Columns] Diameter = 999.99999999999989 (IFCLENGTHMEASURE) [MILLI METRE]
    [Columns] Number of columns = 4 (IFCINTEGER)
    [Columns] Spacing = 11999.999999999998 (IFCLENGTHMEASURE) [MILLI METRE]
    [Columns] Width = 2999.9999999999995 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions: 6 more contents on 6 objects not shown
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    AC135_EhKompleksKlassKood = "R" (IFCTEXT)
    AC140_EhKompleksKlassNimi = "Liikluskompleks" (IFCTEXT)
    AC145_EhitisKlassKood = "RK" (IFCTEXT)
    AC150_EhitisKlassNimi = "Sild" (IFCTEXT)
    Author = "Raido Puust" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 2" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCSLAB)
    AC155_SysteemKlassKood = "C" (IFCTEXT)
    AC156_SysteemTyypKood = "C50" (IFCTEXT)
    AC157_SysteemID = "C5001" (IFCTEXT)
    AC160_SysteemKlassNimi = "Vahelaesüsteem" (IFCTEXT)
    AC161_SysteemTyypNimi = "Silla pealisehituse süsteem" (IFCTEXT)
    AC165_OsasysteemKlassKood = "BC" (IFCTEXT)
    AC166_OsasysteemTyypKood = "BC10" (IFCTEXT)
    AC167_OsasysteemID = "BC1001" (IFCTEXT)
    AC170_OsasysteemKlassNimi = "Talakonstruktsioon" (IFCTEXT)
    AC171_OsaSysteemTyypNimi = "Massiivplaadi konstruktsioon" (IFCTEXT)
    AC175_KomponentKlassKood = "ULK" (IFCTEXT)
    AC176_KomponentTyypKood = "ULK21" (IFCTEXT)
    AC177_KomponentID = "ULK01" (IFCTEXT)
    AC180_KomponentKlassNimi = "Plaat" (IFCTEXT)
    AC181_KomponentTyypNimi = "Betoonvalust plaat" (IFCTEXT)
    AR340_Viitetunnus = "ULK01%ULK21" (IFCTEXT)
    AR360_UnikaalneID = "C5001.BC1001.ULK01%ULK21" (IFCTEXT)
    Class Identifier = 15 (IFCINTEGER)
    Feature Identifier = 1 (IFCINTEGER)
    Name = "Deck 1" (IFCTEXT)
    Unique Identifier = "a0aa66b4-e5b2-40eb-89b9-6a0242144a27-1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCSLAB)
    AC155_SysteemKlassKood = "B" (IFCTEXT)
    AC156_SysteemTyypKood = "B32" (IFCTEXT)
    AC157_SysteemID = "B3201" (IFCTEXT)
    AC160_SysteemKlassNimi = "Seinasüsteem" (IFCTEXT)
    AC161_SysteemTyypNimi = "Toeseina süsteem" (IFCTEXT)
    AC165_OsasysteemKlassKood = "CJ" (IFCTEXT)
    AC166_OsasysteemTyypKood = "CJ10" (IFCTEXT)
    AC167_OsasysteemID = "CJ1001" (IFCTEXT)
    AC170_OsasysteemKlassNimi = "Vundamendi ja aluse konstruktsioon" (IFCTEXT)
    AC171_OsaSysteemTyypNimi = "Tugiseina ehitus" (IFCTEXT)
    AC175_KomponentKlassKood = "ULJ" (IFCTEXT)
    AC176_KomponentTyypKood = "ULJ10" (IFCTEXT)
    AC177_KomponentID = "ULJ01" (IFCTEXT)
    AC180_KomponentKlassNimi = "Kaldtugi" (IFCTEXT)
    AC181_KomponentTyypNimi = "Kaldasammas" (IFCTEXT)
    AR340_Viitetunnus = "ULJ01%ULJ10" (IFCTEXT)
    AR360_UnikaalneID = "B3201.CJ1001.ULJ01%ULJ10" (IFCTEXT)
    Class Identifier = 1 (IFCINTEGER)
    Feature Identifier = 2 (IFCINTEGER)
    Name = "Abutment 2" (IFCTEXT)
    Unique Identifier = "542b763a-2260-4b04-9d50-65004f83fa3a_1_0" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AC155_SysteemKlassKood = "C" (IFCTEXT)
    AC156_SysteemTyypKood = "C50" (IFCTEXT)
    AC157_SysteemID = "C5001" (IFCTEXT)
    AC160_SysteemKlassNimi = "Vahelaesüsteem" (IFCTEXT)
    AC161_SysteemTyypNimi = "Silla pealisehituse süsteem" (IFCTEXT)
    AC165_OsasysteemKlassKood = "BC" (IFCTEXT)
    AC166_OsasysteemTyypKood = "BC20" (IFCTEXT)
    AC167_OsasysteemID = "BC2001" (IFCTEXT)
    AC170_OsasysteemKlassNimi = "Talakonstruktsioon" (IFCTEXT)
    AC171_OsaSysteemTyypNimi = "Tala konstruktsioon" (IFCTEXT)
    AC175_KomponentKlassKood = "UPA" (IFCTEXT)
    AC176_KomponentTyypKood = "UPA70" (IFCTEXT)
    AC177_KomponentID = "UPA12" (IFCTEXT)
    AC180_KomponentKlassNimi = "Laagerdus" (IFCTEXT)
    AC181_KomponentTyypNimi = "Elastomeerne laager" (IFCTEXT)
    AR340_Viitetunnus = "UPA12%UPA70" (IFCTEXT)
    AR360_UnikaalneID = "C5001.BC2001.UPA12%UPA70" (IFCTEXT)
    Class Identifier = 18 (IFCINTEGER)
    Feature Identifier = 14 (IFCINTEGER)
    Name = "Bearing 1" (IFCTEXT)
    Unique Identifier = "ff909951-ccef-4b37-a31b-6f972beeee0b_1_0" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AC155_SysteemKlassKood = "C" (IFCTEXT)
    AC156_SysteemTyypKood = "C50" (IFCTEXT)
    AC157_SysteemID = "C5001" (IFCTEXT)
    AC160_SysteemKlassNimi = "Vahelaesüsteem" (IFCTEXT)
    AC161_SysteemTyypNimi = "Silla pealisehituse süsteem" (IFCTEXT)
    AC165_OsasysteemKlassKood = "BC" (IFCTEXT)
    AC166_OsasysteemTyypKood = "BC20" (IFCTEXT)
    AC167_OsasysteemID = "BC2001" (IFCTEXT)
    AC170_OsasysteemKlassNimi = "Talakonstruktsioon" (IFCTEXT)
    AC171_OsaSysteemTyypNimi = "Tala konstruktsioon" (IFCTEXT)
    AC175_KomponentKlassKood = "UPA" (IFCTEXT)
    AC176_KomponentTyypKood = "UPA70" (IFCTEXT)
    AC177_KomponentID = "UPA11" (IFCTEXT)
    AC180_KomponentKlassNimi = "Laagerdus" (IFCTEXT)
    AC181_KomponentTyypNimi = "Elastomeerne laager" (IFCTEXT)
    AR340_Viitetunnus = "UPA11%UPA70" (IFCTEXT)
    AR360_UnikaalneID = "C5001.BC2001.UPA11%UPA70" (IFCTEXT)
    Class Identifier = 18 (IFCINTEGER)
    Feature Identifier = 15 (IFCINTEGER)
    Name = "Bearing 1" (IFCTEXT)
    Unique Identifier = "6f565c8b-6a57-4516-a57d-07fc603e1d0f_1_0" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AC155_SysteemKlassKood = "C" (IFCTEXT)
    AC156_SysteemTyypKood = "C50" (IFCTEXT)
    AC157_SysteemID = "C5001" (IFCTEXT)
    AC160_SysteemKlassNimi = "Vahelaesüsteem" (IFCTEXT)
    AC161_SysteemTyypNimi = "Silla pealisehituse süsteem" (IFCTEXT)
    AC165_OsasysteemKlassKood = "BC" (IFCTEXT)
    AC166_OsasysteemTyypKood = "BC20" (IFCTEXT)
    AC167_OsasysteemID = "BC2001" (IFCTEXT)
    AC170_OsasysteemKlassNimi = "Talakonstruktsioon" (IFCTEXT)
    AC171_OsaSysteemTyypNimi = "Tala konstruktsioon" (IFCTEXT)
    AC175_KomponentKlassKood = "UPA" (IFCTEXT)
    AC176_KomponentTyypKood = "UPA70" (IFCTEXT)
    AC177_KomponentID = "UPA13" (IFCTEXT)
    AC180_KomponentKlassNimi = "Laagerdus" (IFCTEXT)
    AC181_KomponentTyypNimi = "Elastomeerne laager" (IFCTEXT)
    AR340_Viitetunnus = "UPA13%UPA70" (IFCTEXT)
    AR360_UnikaalneID = "C5001.BC2001.UPA13%UPA70" (IFCTEXT)
    Class Identifier = 18 (IFCINTEGER)
    Feature Identifier = 13 (IFCINTEGER)
    Name = "Bearing 1" (IFCTEXT)
    Unique Identifier = "d05f8f0f-dae7-40a9-b814-e8362617b30f_1_0" (IFCTEXT)
  Identity Data: 44 more contents on 25 objects not shown
  General | properties | on 1 object (1 IFCSLAB)
    CIP concrete volume = 180.62071228027344 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Concrete strength = 34999999.999999993 (IFCPRESSUREMEASURE) [PASCAL]
    Continuity = "Simply supported" (IFCTEXT)
    End station = 571.64659787327014 (IFCREAL)
    Has haunches = FALSE (IFCBOOLEAN)
    Haunch height = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Left edge to curb = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 35729.289174488869 (IFCLENGTHMEASURE) [MILLI METRE]
    Offset from = 0. (IFCREAL)
    Part type = "Component Deck" (IFCTEXT)
    Right edge to curb = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Start station = 535.91801508879144 (IFCREAL)
    Superimposed DL = 914.39999999999998 (IFCTORQUEMEASURE) [derived]
    Wearing surface = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Width: End = 16849.9755859375 (IFCLENGTHMEASURE) [MILLI METRE]
    Width: Start = 16849.9755859375 (IFCLENGTHMEASURE) [MILLI METRE]
  General | properties | on 1 object (1 IFCSLAB)
    Azimuth = 256.82610984009636 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    CIP concrete volume = 313.12173499147997 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Diaphragm width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left overhang = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Part type = "Wing Walls 1" (IFCTEXT)
    Right overhang = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Skew = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Station = 571.64659787327014 (IFCREAL)
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Offset: Lateral = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Offset: Station = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Part type = "Legacy Bearing" (IFCTEXT)
    Rotation: Z = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Station = 570.6657589623585 (IFCREAL)
    Top elevation = 20485.597934573889 (IFCLENGTHMEASURE) [MILLI METRE]
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Offset: Lateral = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Offset: Station = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Part type = "Legacy Bearing" (IFCTEXT)
    Rotation: Z = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Station = 570.66612269931295 (IFCREAL)
    Top elevation = 20448.552013374865 (IFCLENGTHMEASURE) [MILLI METRE]
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Offset: Lateral = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Offset: Station = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Part type = "Legacy Bearing" (IFCTEXT)
    Rotation: Z = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Station = 570.66540217116062 (IFCREAL)
    Top elevation = 20469.562457874414 (IFCLENGTHMEASURE) [MILLI METRE]
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Offset: Lateral = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Offset: Station = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Part type = "Legacy Bearing" (IFCTEXT)
    Rotation: Z = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Station = 570.66503789079161 (IFCREAL)
    Top elevation = 20432.683208957314 (IFCLENGTHMEASURE) [MILLI METRE]
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Offset: Lateral = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Offset: Station = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Part type = "Legacy Bearing" (IFCTEXT)
    Rotation: Z = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Station = 570.66467333983553 (IFCREAL)
    Top elevation = 20395.805029198527 (IFCLENGTHMEASURE) [MILLI METRE]
  General | properties | on 1 object (1 IFCSLAB)
    Azimuth = 257.11701561635169 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    CIP concrete volume = 313.32096242712009 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Diaphragm width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left overhang = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Part type = "Wing Walls 1" (IFCTEXT)
    Right overhang = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Skew = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Station = 535.91801508879144 (IFCREAL)
  General: 22 more contents on 22 objects not shown
  Phasing | properties | on 30 objects (25 IFCBUILDINGELEMENTPROXY, 3 IFCSLAB, 2 IFCCOLUMN)
    Phase Created = "New Construction" (IFCLABEL)
  Structural | properties | on 30 objects (25 IFCBUILDINGELEMENTPROXY, 3 IFCSLAB, 2 IFCCOLUMN)
    Rebar Cover = "Interior (framing, columns) <40 mm>" (IFCLABEL)
  Other(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Constraints(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Center" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)